1. A furnace with an aperture of 20 mm diameter and **emissive power of 3.72×105 W/m2** is used to calibrate a heat flux gage having a sensitive area of 1.6×10−5 m2 . At what distance, measured along the normal direction from the aperture, should the gage be positioned to receive irradiation of 1000 W/m2 ? If the gage is tilted off normal by 20 degrees, what will the irradiation be at this distance?

|  |  |
| --- | --- |
|  |  |

1. On an overcast day the directional distribution of the solar radiation incident on the earth’s surface may be approximated by an expression of the form Ii = In cos θ, where In = 80 W/m2 -sr is the total intensity of radiation directed normal to the surface and θ is the zenith angle. What is the solar irradiation at the earth’s surface?

|  |  |
| --- | --- |
|  |  |

1. Determine the fraction of total, hemispherical emissive power that leaves a diffuse surface for the angle ranges of π/4 ≤ θ ≤ π/2 and 0 ≤ φ ≤ π.


|  |  |
| --- | --- |
|  |  |

1. Assuming the earth’s surface is black, estimate its temperature if the sun has an equivalent blackbody temperature of 5800 K. The diameters of the sun and earth are 1.39 × 109 m and 1.29 × 107 m, respectively, and the distance between the sun and earth is 1.5 × 1011 m.

|  |  |
| --- | --- |
|  |  |

1. Estimate the wavelength corresponding to maximum emission from each of the following surfaces: the sun (5800 K), a tungsten filament (2500 K), a heated metal surface (1500 K), and a cryogenically cooled metal surface (60 K). What fraction of the surface emission is in the ultraviolet (λ ≤ 400 nm), visible (400 nm ≤ λ ≤ 700 nm), and infrared (700 nm ≤ λ) for each surface

|  |  |
| --- | --- |
|  |  |

1. The spectral, hemispherical emissivity of tungsten may be approximated by the distribution depicted below. Consider a cylindrical tungsten filament that is of diameter D = 0.8 mm and length L = 20 mm. The filament is enclosed in an evacuated bulb and is heated by an electrical current to a steady-state temperature of 2900 K. What is the total hemispherical emissivity when the filament temperature is 2900 K? Assuming the surroundings are at 300 K, what is the initial rate of cooling when the current is switched off? 

|  |  |
| --- | --- |
|  |  |